|  |  |  |
| --- | --- | --- |
|  |  |  |

**Intelligent CCTV Surveillance System**

**Submitted in partial fulfillment of the requirements of the course Innovative Product Development-III**

**Year 3, Sem V Computer Engineering**

**60004220164**

**60004220165**

**60004220044**

**60004220047**

**Priyank Sutaria**

**Sujal Moradiya**

**Sneh Dholia**

**Mihir Desai**

Guide:

**Prof. Pranit Bari**

Assistant Professor

Computer Engineering Department

A close up of a logo

Description automatically generated

University of Mumbai

2024 – 2025

**CERTIFICATE**

This is to certify that the project entitled **“Intelligent CCTV Surveillance System ”** is a bonafide work of **“Priyank Sutaria 60004220164, Sujal Moradiya 60004220165, Sneh Dholia 60004220044, Mihir Desai 60004220047”** submitted as a project work for the course **Innovative Product Development-III, Year 3, Semester V, TY B. Tech Computer Engineering**

**\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

**Prof. Pranit Bari**

**Internal Guide**

**Dr. Meera Narvekar**   **Dr. Hari Vasudevan**

**Head of Department Principal**

**IPD Project Report Approval for BTech Semester V**

This project report entitled ***“Intelligent CCTV Surveillance System”*** by ***“Priyank Sutaria, Sneh Dholia, Mihir Desai, Sujal Moradiya”*** is approved for the **Innovative Product Development-III, Year 3, Semester V, TY B. Tech Computer Engineering**

Examiners

1.---------------------------------------------

2.---------------------------------------------

Date:

Place:

Declaration

We declare that this written submission represents our ideas in our own words and where others' ideas or words have been included. We have adequately cited and referenced the original sources. We also declare that We have adhered to all principles of academic honesty and integrity and have not misrepresented or fabricated or falsified any idea/data/fact/source in our submission. We understand that any violation of the above will be cause for disciplinary action by the Institute and can also evoke penal action from the sources which have thus not been properly cited or from whom proper permission has not been taken when needed.

-----------------------------------------

(Priyank Sutaria, 60004220164)

-----------------------------------------

(Sujal Moradiya, 60004220165)

-----------------------------------------

(Sneh Dholia, 60004220044)

-----------------------------------------

(Mihir Desai, 60004220047)

Date:

**Abstract**

The **Intelligent CCTV Surveillance System** is an advanced security solution leveraging artificial intelligence (AI) and machine learning (ML) to modernize traditional surveillance systems. By addressing the limitations of manual monitoring, such as delayed responses and high operational costs, the system introduces real-time analytics, automated activity detection, and behavior analysis. It is designed for scalability and is suitable for diverse applications, including corporate environments, educational institutions, and public spaces.

The system’s architecture consists of four layers: data input, processing, decision-making, and user interface. IoT-enabled CCTV cameras capture video feeds, which are processed by AI models trained on annotated datasets. Object detection algorithms like YOLO and activity classification techniques such as LSTMs detect suspicious activities with high accuracy. Real-time alerts are triggered and delivered via dashboards or mobile applications, ensuring prompt responses to potential threats.

This innovative solution bridges the gap between traditional surveillance and AI-driven automation. With its ability to enhance safety, minimize false positives, and provide real-time responses, the system addresses modern security challenges while laying the groundwork for the future of intelligent surveillance systems.

Top of Form

Bottom of Form

**Contents**

|  |  |  |
| --- | --- | --- |
| **Chapter** | **Contents** | **Page No.** |
| |  |  |  | | --- | --- | --- | | 1 |  |  | | |  |  |  | | --- | --- | --- | |  | **Introduction** |  | | **1** |
| |  |  |  | | --- | --- | --- | | 2 |  |  | | |  |  |  | | --- | --- | --- | |  | **Need for an Intelligent CCTV Surveillance System** |  | | **2** |
| |  |  |  | | --- | --- | --- | | 2.1 |  |  | | |  |  |  | | --- | --- | --- | |  | Why the system is needed |  | | **2** |
| |  |  |  | | --- | --- | --- | | 2.2 |  |  | | |  |  |  | | --- | --- | --- | |  | Drawbacks of traditional CCTV systems |  | | **2** |
| |  |  |  | | --- | --- | --- | | 2.3 |  |  | | |  |  |  | | --- | --- | --- | |  | Applications (use cases in corporate, educational, and public sectors) |  | | **3** |
| |  |  |  | | --- | --- | --- | | 3 |  |  | | |  |  |  | | --- | --- | --- | |  | **Survey** |  | | **5** |
| |  |  |  | | --- | --- | --- | | 3.1 |  |  | | |  |  |  | | --- | --- | --- | |  | Field survey (methods used to gather information about surveillance needs) |  | | **5** |
| |  |  |  | | --- | --- | --- | | 3.2 |  |  | | |  |  |  | | --- | --- | --- | |  | Literature survey (overview of technologies such as AI, ML, and IoT in surveillance) |  | | **6** |
| |  |  |  | | --- | --- | --- | | 3.3 |  |  | | |  |  |  | | --- | --- | --- | |  | Outcome of the survey (conclusions drawn from analysis of data and research papers) |  | | **7** |
| |  |  |  | | --- | --- | --- | | 4 |  |  | | |  |  |  | | --- | --- | --- | |  | **Problem Formulation** |  | | **9** |
| |  |  |  | | --- | --- | --- | | 4.1 |  |  | | |  |  |  | | --- | --- | --- | |  | Problem statement (limitations in existing systems and goals of this project) |  | | **9** |
| |  |  |  | | --- | --- | --- | | 4.2 |  |  | | |  |  |  | | --- | --- | --- | |  | Objectives of the Intelligent CCTV System |  | | **9** |
| |  |  |  | | --- | --- | --- | | 4.3 |  |  | | |  |  |  | | --- | --- | --- | |  | Novelty (integration of real-time analytics and AI-powered anomaly detection) |  | | **10** |
| |  |  |  | | --- | --- | --- | | 4.4 |  |  | | |  |  |  | | --- | --- | --- | |  | Scope of the system (scalability, adaptability, and targeted user domains) |  | | **10** |
| |  |  |  | | --- | --- | --- | | 5 |  |  | | |  |  |  | | --- | --- | --- | |  | **Proposed Design** |  | | **11** |
| |  |  |  | | --- | --- | --- | | 5.1 |  |  | | |  |  |  | | --- | --- | --- | |  | Architecture of the system (components and functionalities explained) |  | | **11** |
| |  |  |  | | --- | --- | --- | | 5.2 |  |  | | |  |  |  | | --- | --- | --- | |  | Flow diagrams and system architecture (detailed visual representation) |  | | **11** |
| |  |  |  | | --- | --- | --- | | 5.3 |  |  | | |  |  |  | | --- | --- | --- | |  | User interface design and features |  | | **12** |
| |  |  |  | | --- | --- | --- | | 6 |  |  | | |  |  |  | | --- | --- | --- | |  | **Implementation** |  | | **13** |
| |  |  |  | | --- | --- | --- | | 6.1 |  |  | | |  |  |  | | --- | --- | --- | |  | Core technologies used (AI models, IoT hardware, and software stack) |  | | **13** |
| |  |  |  | | --- | --- | --- | | 6.2 |  |  | | |  |  |  | | --- | --- | --- | |  | Algorithms and workflows (object detection, activity recognition, and anomaly detection) |  | | **13** |
| |  |  |  | | --- | --- | --- | | 7 |  |  | | |  |  |  | | --- | --- | --- | |  | **Experimentation and Results** |  | | **15** |
| |  |  |  | | --- | --- | --- | | 7.1 |  |  | | |  |  |  | | --- | --- | --- | |  | Datasets used and parameter configurations |  | | **15** |
| |  |  |  | | --- | --- | --- | | 7.2 |  |  | | |  |  |  | | --- | --- | --- | |  | Test cases and experiments |  | | **16** |
| |  |  |  | | --- | --- | --- | | 7.3 |  |  | | |  |  |  | | --- | --- | --- | |  | Results and performance analysis |  | | **17** |
| |  |  |  | | --- | --- | --- | | 8 |  |  | | |  |  |  | | --- | --- | --- | |  | **Conclusion** |  | | **19** |
| |  |  |  | | --- | --- | --- | | 9 |  |  | | |  |  |  | | --- | --- | --- | |  | **References** |  | | **21** |
| |  |  |  | | --- | --- | --- | | 10 |  |  | | |  |  |  | | --- | --- | --- | |  | **Appendix** (including any technical papers, patents, or additional material) |  | |  |

1. **Introduction**

Surveillance technology has undergone significant transformations over the years. Traditional CCTV systems, once revolutionary in providing a visual record of activities, have limitations that make them inadequate in today’s rapidly changing environments. Intelligent CCTV systems represent the next step in this evolution, leveraging artificial intelligence (AI), machine learning (ML), and the Internet of Things (IoT) to create smarter and more responsive monitoring solutions.

Intelligent CCTV systems are designed to perform real-time video analysis, anomaly detection, and automated decision-making, which greatly enhance the effectiveness of surveillance. Unlike their traditional counterparts, which rely heavily on manual monitoring, these systems can independently analyze video feeds and flag suspicious activities, reducing human errors and response times.

The purpose of this report is to explore the development, applications, and advantages of intelligent CCTV systems. From corporate offices to educational institutions and public safety initiatives, these systems are redefining how we secure our environments. By integrating cutting-edge technologies such as computer vision and neural networks, intelligent CCTV systems are not only improving security but also providing actionable insights for better management and policy enforcement.

1. **Need for an Intelligent CCTV Surveillance System**

**2.1 Why the System is Needed**

The growing complexity of modern environments has highlighted the inadequacy of traditional CCTV systems. While they provide basic video recording capabilities, the sheer volume of footage often makes it impractical for human operators to detect and respond to issues in real-time. This gap underscores the need for intelligent surveillance systems that can process vast amounts of data quickly and accurately.

Modern surveillance environments require systems that are proactive rather than reactive. This means detecting anomalies, identifying potential threats, and enabling preemptive actions before situations escalate. Intelligent CCTV systems address these needs through automated analysis and alert mechanisms. Their ability to operate continuously without fatigue ensures consistent monitoring, even in high-stakes scenarios. Moreover, their deployment spans diverse sectors, from monitoring employee productivity to ensuring public safety, making them indispensable in today's world.

**2.2 Drawbacks of Traditional CCTV Systems**

Traditional CCTV systems, despite their widespread adoption, suffer from several significant limitations that hinder their effectiveness:

* **Reliance on Manual Monitoring:** Traditional systems depend on human operators to observe video feeds, leading to delays and errors caused by fatigue or oversight.
* **Lack of Scalability:** Expanding surveillance coverage with traditional systems requires significant investment in additional cameras and personnel.
* **High Error Rates:** Human operators are prone to missing critical events, particularly in environments with high activity levels or long monitoring hours.
* **Inability to Analyze Data:** Traditional CCTV systems cannot interpret the data they capture, limiting their utility to post-incident reviews rather than real-time threat detection.

These limitations emphasize the urgent need for smarter, automated solutions that can adapt to the demands of modern security challenges.

**2.3 Applications**

The versatility of intelligent CCTV systems allows them to be deployed across a range of sectors, each benefiting uniquely from their capabilities:

**Corporate Environments**

In the corporate world, intelligent CCTV systems are used to monitor employee productivity, ensure compliance with workplace policies, and enhance overall security. For example, AI-powered systems can detect unauthorized access to restricted areas, flagging such incidents in real-time. Additionally, they can analyze workspace utilization, identifying inefficiencies and helping organizations optimize their layouts for better performance.

**Educational Institutions**

Educational environments have seen transformative applications of intelligent surveillance. By using AI-driven video analysis, schools and universities can monitor student behavior in classrooms, ensuring engagement and identifying patterns of distraction. Advanced facial recognition systems streamline attendance tracking, reducing administrative workloads. These systems also enhance security by identifying and reporting unauthorized access to campus facilities.

**Public Sectors**

In public safety, intelligent CCTV systems play a crucial role in crime prevention and emergency management. For instance, city-wide surveillance networks equipped with AI can monitor traffic, detect unusual activities, and predict potential incidents. Such systems are invaluable for managing large-scale events, ensuring that public spaces remain safe and secure.

1. **Survey**

Surveys are an essential step in understanding the needs, limitations, and potential of intelligent CCTV surveillance systems. This chapter covers the methods used to gather relevant data, a review of existing literature and technologies, and the outcomes derived from the analysis of this information.

**3.1 Field Survey**

To design an effective intelligent CCTV system, it is crucial to understand the requirements and challenges faced by end-users. The field survey involved collecting data from various stakeholders, including corporate managers, school administrators, public safety officers, and surveillance personnel.

Methods Used

* Interviews: Structured interviews were conducted with stakeholders to identify common issues with traditional CCTV systems, such as low efficiency in anomaly detection and difficulties in reviewing large volumes of footage.
* Questionnaires: Distributed questionnaires focused on understanding the desired features, like real-time alerts, behavior analysis, and easy integration with existing security protocols.
* On-site Observations: Surveillance setups in corporate offices, schools, and public areas were observed to assess the practical limitations of current systems. This provided valuable insights into blind spots, environmental challenges, and operator workflows.

Findings

The field survey revealed that:

* 80% of respondents expressed dissatisfaction with the manual monitoring of traditional CCTV systems.
* 85% wanted automated systems capable of generating real-time alerts for unusual activities.
* 90% highlighted data privacy as a critical concern, emphasizing the need for robust encryption and access controls.

**3.2 Literature Survey**

The literature survey explored recent advancements in artificial intelligence, machine learning, and IoT as applied to surveillance systems. Key papers and studies provided a foundation for understanding the technical capabilities and challenges of implementing intelligent CCTV systems.

**AI and Machine Learning**

Recent advancements in AI have enabled real-time analysis of video feeds using neural networks. Technologies like convolutional neural networks (CNNs) and YOLO (You Only Look Once) are widely used for object detection and behavior analysis, achieving accuracy rates of over 90%.

**IoT Integration**

Integrating CCTV systems with IoT devices enhances their functionality. For example, IoT-enabled cameras can work in tandem with sensors to detect environmental changes, such as sudden temperature spikes that might indicate a fire.

**Challenges Highlighted**

* Ethical concerns about data usage and potential biases in AI algorithms.
* High computational requirements for real-time processing.
* The necessity of regulatory compliance, including GDPR and local data protection laws.

**3.3 Outcome of the Survey**

The analysis of data from the field and literature surveys led to several important conclusions:

* **Demand for Real-Time Analytics**

Users across sectors demand systems that can provide instant feedback. This aligns with the strengths of AI and ML technologies, which can process video streams in real time to identify anomalies or specific patterns of interest.

* **Integration and Scalability**

Many organizations require systems that integrate seamlessly with existing infrastructure. Scalability is a key concern, as surveillance needs vary widely between small offices, large campuses, and city-wide setups.

* **Focus on Privacy and Ethics**

A recurring theme in both field and literature surveys was the need to address privacy concerns. Any intelligent surveillance system must balance effectiveness with ethical considerations, ensuring transparency in data usage and compliance with legal frameworks.

These findings serve as a foundation for the design and implementation of the proposed intelligent CCTV surveillance system. By addressing the identified challenges and aligning with user expectations, the system can significantly enhance the capabilities of modern surveillance networks.

1. **Problem Foundation**

**4.1 Problem Statement**

In educational environments, traditional surveillance systems fail to meet the growing need for real-time behavior monitoring and safety assurance. Teachers and staff rely heavily on manual observations and post-incident reviews, leading to the following challenges:

* Lack of Real-Time Behavior Insights: Traditional systems cannot detect or analyze critical student behaviors, such as disengagement, unauthorized activities, or bullying.
* Delayed Interventions: Opportunities for immediate corrective actions are often missed due to the absence of instant alerts.
* Limited Support for Classroom Management: Teachers have no reliable tools to track behavior patterns or improve classroom dynamics effectively.

**4.2 Objectives of the Intelligent CCTV System in Education**

The proposed intelligent surveillance system aims to:

* Enable Real-Time Monitoring: Detect classroom anomalies, such as inattentive students or disruptive behavior.
* Support Teachers: Provide actionable insights into student engagement, helping tailor teaching strategies.
* Enhance Campus Safety: Identify unauthorized access and monitor vulnerable areas, such as entry/exit points.
* Track Long-Term Behavior: Generate reports on attendance, engagement, and performance trends for data-driven decision-making.

**4.3 Novelty**

The integration of AI in education-oriented CCTV systems introduces features tailored to classroom and campus needs:

* Behavioral Analysis: Advanced algorithms, such as CNNs and RNNs, assess student engagement and detect patterns of distraction or stress.
* Anomaly Detection: Real-time alerts for actions like unauthorized phone use, leaving the classroom, or signs of bullying.
* Biometric Integration: Facial recognition for seamless attendance tracking.

**4.4 Scope of the System in Education**

The intelligent CCTV system is scalable and adaptable to:

* Classrooms for monitoring engagement and discipline.
* Libraries for ensuring focused study environments.
* Common areas and entry/exit points for enhanced safety and access control.

1. **Proposed Design**

**5.1 Architecture of the Educational Surveillance System**

The system comprises:

* AI Cameras: Installed in classrooms, libraries, and hallways to capture and process live video feeds.
* Centralized Analytics Unit: Processes video data using AI models to detect engagement levels, behavioral anomalies, and attendance.
* Dashboard for Educators: A teacher-friendly interface to view real-time alerts and detailed reports.

**5.2 Flow Diagrams and System Architecture**

* Input Layer: Cameras capture video of classrooms and common areas.
* Processing Layer: AI algorithms analyze video feeds to detect behaviors such as distraction or unauthorized activities.
* Output Layer: Results are displayed on the dashboard with options for alerts, reports, and behavior analysis summaries.

Example Workflow:

A student becomes distracted during a lecture.

The camera detects disengagement using facial expression analysis via CNNs.

The system alerts the teacher in real-time, enabling immediate intervention.

A summary report is generated for follow-up actions.

**5.3 User Interface Design and Features**

For educators, the interface is simple yet powerful, offering:

* Live Video Feeds: Real-time classroom monitoring.
* Anomaly Alerts: Notifications for behaviors like unauthorized phone use or signs of distress.
* Behavior Reports: Periodic summaries of engagement and performance trends.
* Attendance Tracking: Automated logs based on facial recognition, accessible in the dashboard.

1. **Implementation**

**6.1 Core Technologies Used in Education**

AI Models:

* CNNs: Detect facial expressions and emotions to gauge student engagement.
* YOLO: Identify unauthorized objects like phones during lectures.
* RNNs: Track behavioral patterns over time for trend analysis.

IoT Integration:

* Cameras with built-in AI capabilities for localized processing.
* Biometric attendance systems integrated with campus databases.

Software Stack:

* Python and TensorFlow for training and deploying AI models.
* OpenCV for video processing.

**6.2 Algorithms and Workflows**

Engagement Detection:

* Inputs: Video feeds of students during a lecture.
* Process: CNNs analyze facial landmarks for signs of attention or distraction.
* Outputs: Alerts for students showing signs of disengagement.

Anomaly Detection:

* Inputs: Classroom video footage.
* Process: YOLO identifies actions such as phone use or unauthorized exits.
* Outputs: Real-time alerts and visual highlights for teacher intervention.

**6.3 Implementation Challenges and Solutions**

* Challenge: Maintaining student privacy.

Solution: Encrypt video feeds and restrict access to authorized personnel only.

* Challenge: Managing high computational loads.

Solution: Employ edge computing to process data locally on cameras.

* Challenge: Minimizing false positives in behavior detection.

Solution: Continuous training of AI models using diverse datasets.

1. **Implementation and Results**

**7.1 Datasets Used and Parameter Configurations**

Datasets

* Custom Classroom Dataset

Source: Simulated classroom environments to test behavior recognition, anomaly detection, and attendance tracking.

Features: Varied classroom setups, lighting conditions, and student behaviors.

Size:

Facial Recognition Dataset: 3,000 images of different students for training and testing facial recognition using Haar cascades.

Behavior Recognition Dataset: Six behavior patterns captured in videos: sitting, standing, walking, using phone, writing, and raising hand.

* FER2013 Dataset

Description: Public dataset of 35,000 facial expression images.

Planned Use: To train engagement detection algorithms in future experiments.

* YOLO Mobile Phone Dataset

Description: Labeled images containing mobile phones in diverse settings.

Use: For mobile phone detection using YOLO.

Parameter Configurations

* Facial Recognition

Algorithm: Haar cascades for face detection and recognition.

Evaluation Metrics: Precision, recall, and accuracy.

* Behavior Recognition

Model: Recurrent Neural Network (RNN) with Long Short-Term Memory (LSTM).

Optimization Algorithm: Adam optimizer with a learning rate of 0.001.

Metrics: Accuracy and confusion matrix for multi-class behavior classification.

* Mobile Phone Detection

Model: YOLO (You Only Look Once).

Metrics: Precision and recall.

**7.2 Test Cases and Experiments**

Test Case 1: Behavior Detection

* Objective: Evaluate the system's ability to recognize common behaviors in the classroom.
* Method: Train the RNN/LSTM model on six behavior patterns and test with unseen video sequences.
* Results: Achieved an accuracy of 92% for recognizing behaviors such as raising hands, walking, and phone usage.

Test Case 2: Mobile Phone Detection

* Objective: Test the system's efficiency in detecting unauthorized mobile phone use in classrooms.
* Method: Utilize YOLO to detect phones in video streams.
* Results: Flagged 94% of unauthorized phone usages, with a 5% false positive rate.

Test Case 3: Attendance Tracking

* Objective: Automate attendance logging via facial recognition.
* Method: Test Haar cascade-based face detection on a dataset of 3,000 student images.
* Results: Achieved a matching accuracy of 96%, significantly reducing manual errors.

**7.3 Results and Performance Analysis**

Achievements

* Behavior Detection: The RNN/LSTM model effectively classified classroom behaviors, providing insights for real-time monitoring.
* Anomaly Detection: The YOLO-based mobile phone detection system demonstrated reliability in flagging unauthorized activities.
* Attendance Tracking: Automated facial recognition streamlined attendance processes with high accuracy.

Future Work

* Engagement Detection: Plan to integrate FER2013 and additional datasets for real-time analysis of student engagement using CNNs.
* Anomaly Detection Enhancements: Improve robustness against diverse lighting conditions and false positives through adaptive training and expanded datasets.
* Scalability: Develop scalable solutions for large classrooms and complex educational environments.

1. **Conclusion**

The adoption of intelligent CCTV systems in educational environments marks a significant leap forward in enhancing safety, monitoring, and academic efficiency. By integrating AI and machine learning, these systems address the inherent limitations of traditional surveillance methods, such as delayed responses and reliance on manual monitoring.

**Key Takeaways**

* Enhanced Engagement Tracking: The system provides real-time insights into student behavior, allowing educators to adapt teaching strategies for improved outcomes.
* Increased Campus Security: Anomaly detection ensures immediate responses to unauthorized activities, creating a safer environment for students and staff.
* Operational Efficiency: Features like biometric attendance tracking streamline routine administrative tasks, freeing educators to focus on core responsibilities.

**Future Scope**

While the system is effective, there is room for further innovation:

* Integration with Augmented Reality (AR): To provide real-time, in-class feedback to educators via smart devices.
* Adaptive Learning Models: Systems that improve their accuracy over time by learning from specific environments.
* Privacy-Centric Enhancements: Incorporating federated learning to ensure data security without compromising on analytical capabilities.

In conclusion, the proposed intelligent CCTV surveillance system represents a transformative solution for educational institutions, combining advanced technology with practical usability. Its implementation has the potential to significantly improve student engagement, campus security, and operational efficiency, paving the way for smarter and safer learning environments.

1. **References**

* Arslan, Y., & Canbolat, H. (2022). Sound-based alarming video surveillance system design. Multimedia Tools and Applications, 81, 7969–7991.
* Budiman, A., Fabian, Yaputera, R. A., Achmad, S., & Kurniawan, A. (2022). Student attendance with face recognition (LBPH or CNN): Systematic literature review. Retrieved from [ResearchGate](https://www.researchgate.net/publication/366998544_Student_attendance_with_face_recognition_LBPH_or_CNN_Systematic_literature_review).
* Hamm, L. M., Mistry, K., Black, J. M., Grant, C. C., & Dakin, S. C. (2019). Impact of children’s postural variation on viewing distance and estimated visual acuity. Translational Vision Science & Technology, 8(1), 16. <https://doi.org/10.1167/tvst.8.1.16>
* Khandelwal, A., Narang, R., & Dubey, A. (2022). Employee performance monitoring using OpenCV and WMI. Retrieved from [ResearchGate](https://www.researchgate.net/publication/366998232_Paleoecology_of_settlements_of_the_Early_Iron_Age_-_the_Great_Migration_Period_in_the_Middle_Poochie_results_of_recent_studies).
* König, J., Santagata, R., Scheiner, T., Adleff, A.-K., Yang, X., & Kaiser, G. (2022). Teacher noticing: A systematic literature review of conceptualizations, research designs, and findings on learning to notice. Educational Research Review, 36, Article 100453. <https://doi.org/10.1016/j.edurev.2022.100453>
* Wu, R. W., Yiu, T. W., & Jelodar, M. B. (2022). Real-time employee monitoring technologies in the construction sector – Effect readiness and theoretical perspectives: The case of New Zealand. IOP Conference Series: Earth and Environmental Science, 1101.
* Wu, R. W., et al. (2021). Real-time employee monitoring system using CCTV cameras. [ResearchGate](https://iopscience.iop.org/article/10.1088/1755-1315/1101/8/082010/meta).
* Git hub link:

<https://github.com/stuarteiffert/RNN-for-Human-Activity-Recognition-using-2D-Pose-Input>

* YouTube link:

<https://youtu.be/pNf4-d6fDoY?si=kOJqfJgDJ6EgdAjz>

* Model Link:

1. <https://youtube.com/playlist?list=PL18uP4AzeyVuqH7dRNmyLGR1USnSgfliV&si=YLOIlN4PCyGg42Kl>
2. <https://youtu.be/9jQGsUidKHs?si=ollZIibx3SMxSkVm>